**Sound absorber box SB 12/16**

Sound absorber box for ventilation systems.

Connection for DN 125 folded spiral-seams duct with SVR 125 plug connector.

Connection for DN 160 directly on EPP sockets. Seal provided by the customer.

Made from sound-absorbing polypropylene (EPP) with hygienic fleece lamination.

With sound absorbing cover made from melamine resin foam free from mineral fibres.

Two service openings.

With pre-drilled holes for installation with threaded rods.

Technical data

|  |  |
| --- | --- |
| Article: | SB 12/16 |
| Material: | Plastic EPP |
| Weight: | 1,74 kg |
| Weight including packaging: | 1,77 kg |
| Width: | 435 mm |
| Height: | 365 mm |
| Depth: | 220 mm |
| Width with packaging: | 645 mm |
| Height with packaging: | 370 mm |
| Depth with packaging: | 225 mm |
| Insertion loss at 63 Hz: | 2 dB |
| Insertion loss at 125 Hz: | 8 dB |
| Insertion loss at 250 Hz: | 12 dB |
| Insertion loss at 500 Hz: | 20 dB |
| Insertion loss at 1 kHz: | 38 dB |
| Insertion loss at 2 kHz: | 47 dB |
| Insertion loss at 4 kHz: | 40 dB |
| Insertion loss at 8 kHz: | 35 dB |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799599951 |
| Article number: | 0059.0995 |

Manufacturer: MAICO

SB 12/16 Sound absorber box