**Exhaust and supply air valve AZV 100**

Alternative to the disk valve.

Minimum pressure loss.

Continuously variable air flow control via setting screw.

Can be set quickly, easily and precisely.

The grille setting is retained even once the grille has been removed (for cleaning) and re-inserted.

High-quality design for the domestic area.

Covered filter keeps the duct clean.

ISO Coarse 30 % (G2) filter and sealing strip not included in scope of delivery.

The filter is washable.

Alternatively, an ISO Coarse 45 % (G3) filter can be used.

Accessories:

ALDF 125/160 G2 replacement air filter

ALDF 125/160 G3 replacement air filter

Technical data

|  |  |
| --- | --- |
| Article: | AZV 100 |
| Air direction: | Ventilation and air extraction |
| Installation: | Inside |
| Installation site: | Wall |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,29 kg |
| Weight including packaging: | 0,38 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Suitable for nominal size: | 100 mm |
| Width: | 160 mm |
| Height: | 160 mm |
| Depth: | 85 mm |
| Width with packaging: | 170 mm |
| Height with packaging: | 170 mm |
| Depth with packaging: | 110 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799520870 |
| Article number: | 0152.0087 |

Manufacturer: MAICO

AZV 100 Exhaust and supply air valve