**Insulated wall block PP 45 MB**

Wall block with very good thermal insulation for holding DN 160 wall sleeves.

Takes the place of the core hole in new builds.

As optional accessory for holding the PP 45 RHK and/or PP 45 RHL shell sleeve and outside air openings in DN 160.

The installation depth of 365 mm can be shortened to 300 mm or 240 mm using the integrated cutting marks.

Can be extended to any length using further PP 45 MB wall blocks.

Fire-proof class B1.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 MB |
| Installation site: | Outside wall |
| Material: | Plastic EPP |
| Colour: | Black |
| Weight: | 0,67 kg |
| Weight including packaging: | 0,71 kg |
| Fire protection: | Fire-proof class B1 |
| Nominal size: | 180 mm |
| Width: | 248 mm |
| Height: | 248 mm |
| Depth: | 365 mm |
| Width with packaging: | 255 mm |
| Height with packaging: | 255 mm |
| Depth with packaging: | 375 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799581437 |
| Article number: | 0058.0143 |

Manufacturer: MAICO

PP 45 MB Insulated wall block