**Air quality controller Trio VOC I**

The VOC sensor controls the ventilation system on the basis of volatile organic compounds (VOCs) present.

The sensor’s measuring range is 0 – 100% (in relation to calibration gas).

Control range is set in the factory to 30-100%.

Technical data

|  |  |
| --- | --- |
| Article: | Trio VOC I |
| Rated voltage: | 24 V |
| Electrical connection: | Screw terminals |
| Sensor: | internal |
| Weight: | 0,04 kg |
| Weight including packaging: | 0,05 kg |
| Width: | 82 mm |
| Height: | 54 mm |
| Depth: | 25 mm |
| Width with packaging: | 93 mm |
| Height with packaging: | 55 mm |
| Depth with packaging: | 30 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799991175 |
| Article number: | 0157.1483 |

Manufacturer: MAICO

Trio VOC I Air quality controller