**Final assembly kit PPB 30 O**

Approvals and certificates

Test report in accordance with EN 13141-8.

Entry in TZWL bulletin.

Heat exchanger

Thanks to the high-performance heat exchangers and high-efficiency EC fans, the units achieve a degree of heat provision of 73 % at reference volumetric flow according to EN 13141-8.

Installation instructions

Mounting involves 2 steps:

Installation of the PP 45 RHK (DN 160) or PP 45 RHL (DN 160) shell sleeve and an external cover in a DN 160 core drill hole with an inclination of 1-2 %.

We recommend drilling a DN 182 core hole and using the polystyrene shims provided to align the inclination of the sleeve.

The shell sleeve is protected from contamination by plaster protective covers.

Then the final assembly kit is integrated.

No ducts have to be laid and the system does not have to be adjusted.

Electrical connection

When delivered, the unit is assembled and ready for service.

The electrical connection is made using a plug connection.

Connection to RLS 45 K or RLS 45 O room air control using pluggable control cables.

The 12 VDC power cable of the RLS 45 K / RLS 45 O room air control to the unit is also the control cable.

Condensation drain

The condensate is removed via an integrated condensation drip edge in the external cover.

Special features

The PPB 30 O unit is a perfect alternative to ensure cost-effective air extraction in the bathroom with heat recovery. One low-cost solution for a bathroom could be a combination of 1 x PPB 30 O + 1 x RLS 45 O. (Notice: the room air control has the IP 00 degree of protection). An exhaust air mode of 45 m³/h (without heat recovery and without volumetric flow compensation) is also possible.

The PPB 30 O units are primarily designed for installation in the exhaust air rooms. The IP X4 degree of protection facilitates the choice of installation location in the bathroom.

The energy efficiency of the PPB 30 O is impressive with an SPI value of 0.19 Wh/m³.

Due to the energy-saving motors and a very good sensor-guided operation, the devices achieve energy efficiency class A.

The PPB 30 O unit can be operated in 5 ventilation levels 5/12/18/22/26 m³/h and 2 operating modes (continuous ventilation with heat recovery, cross-ventilation without heat recovery).

Flow-optimised external covers in the accessories range keep the exhaust air away from the external façade.

Features

Final installation kits for PushPull Balanced PPB 30 single-room ventilation unit with two fans, two ceramic heat exchangers, internal cover and two integrated ISO Coarse 45 %(G3) filters such that the air is filtered in both directions.

Required accessories

PP 45 RHK or PP 45 RHL shell sleeve

PPB 30 AK, PPB 30 AE, PPB 30 AW or PPB 30 AS external cover

RLS 45 K or RLS 45 O room air control. An RLS 45 K or RLS 45 O room air control can be used to construct a wired ventilation system comprising PPB 30 and PP 45 units. The maximum number of fans used is 6. Thus, different combinations are possible, e.g. 3 x PPB 30 O + 1 x RLS 45 K or 3 x PPB 30 O + 1 x RLS 45 O.

Optional accessories

PPB 30 VS extension kit

PP 45 MB wall block

PPB 30 ARE and PPB 30 ARW compensating frames

PPB 30 ARE BB and PPB 30 ARW BB fixing plates for compensating frame

PP 45 HYI and PP 45 HY humidity sensor

PP 45 CO2 CO2 sensor

PP 45 VOC sensor

Air filter, PPB 30 G3 replacement

Technical data

|  |  |
| --- | --- |
| Article: | PPB 30 O |
| Model: | Object version |
| Air flow volume: | 5 m³/h / 12 m³/h / 18 m³/h / 22 m³/h / 26 m³/h |
| SEC average: | -33,1 kWh/(m²\*a) |
| Energy efficiency class: | A |
| Rated voltage: | 12 V DC |
| SPI value in accordance with DIN EN 13141-8: | 0,19 Wh/m³ |
| Maximum power consumption: | 1,7 W / 2,5 W / 3,4 W / 4,4 W / 5,3 W |
| Degree of protection: | IP X4 |
| Installation position: | horizontal |
| System type: | Decentralised |
| Material: | Synthetic material |
| Housing material: | Synthetic material |
| Heat exchanger material: | Ceramic |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 4,63 kg |
| Weight including packaging: | 5,7 kg |
| Type of filter: | Outside and exhaust air filter |
| Filter class: | ISO Coarse 45 % (G3) |
| Connection diameter: | 160 mm |
| Width: | 275 mm |
| Height: | 275 mm |
| Depth: | 410 mm |
| Width with packaging: | 305 mm |
| Height with packaging: | 325 mm |
| Depth with packaging: | 490 mm |
| Wall has to be broken through: | 162 to 182 mm |
| Degree of heat provision with reference volumetric flow according to DIN EN 13141-8: | 73,3 % |
| Required room air control: | RLS 45 K or RLS 45 O |
| Sound pressure level: | 23 dB(A) / 35 dB(A) / 43 dB(A) / 48 dB(A) / 51 dB(A) Distance 1 m, free-field conditions |
| Rated max. element normal difference in noise level Dn,w: | 37 dB |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799952459 |
| Article number: | 0095.0245 |

Manufacturer: MAICO

PPB 30 O Final assembly kit