**CO2 sensor Trio CO2 I**

The CO2 sensor can be used to control the ventilation system on the basis of the measured CO2 value.

The sensor’s measuring range is 0 – 2000 ppm.

The control range is set in the factory to 600 – 1300 ppm.

Technical data

|  |  |
| --- | --- |
| Article: | Trio CO2 I |
| Sensor: | internal |
| Colour: | grey |
| Weight: | 0,03 kg |
| Weight including packaging: | 0,1 kg |
| Width: | 44,5 mm |
| Height: | 18 mm |
| Depth: | 70 mm |
| Width with packaging: | 50 mm |
| Height with packaging: | 20 mm |
| Depth with packaging: | 75 mm |
| Ambient temperature: | -40 °C up to 70 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799991304 |
| Article number: | 0157.1332 |

Manufacturer: MAICO

Trio CO2 I CO2 sensor