**Air quality controller Trio VOC E**

The VOC sensor controls the ventilation system on the basis of the volatile organic compounds present.

The sensor’s measuring range is 0 – 100 %.

The control range is set in the factory to 30 – 100 %.

Technical data

|  |  |
| --- | --- |
| Article: | Trio VOC E |
| Rated voltage: | 24 V AC / DC |
| Electrical connection: | Screw terminals |
| Sensor: | External |
| Weight: | 0,07 kg |
| Weight including packaging: | 0,1 kg |
| Width: | 82 mm |
| Height: | 82 mm |
| Depth: | 25 mm |
| Width with packaging: | 85 mm |
| Height with packaging: | 85 mm |
| Depth with packaging: | 30 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799991380 |
| Article number: | 0157.1510 |

Manufacturer: MAICO

Trio VOC E Air quality controller