**Roof outlet sleeve PP 45 DFHK**

Roof outlet sleeve for installation in heat-insulated PP 45 DFK roof outlet duct with an incline of 1-2 %.

Accessory needed for PP 45 K, PP 45 O, PP 45 RC, PPB 30 K and PPB 30 O final installation kits when mounting in pitched roofs.

Scope of delivery: 1 x shell sleeve, 1 x mounting material.

A roof outlet kit comprising 1-2 roof outlet ducts, 1x short or long roof outlet sleeve, 1x roof cover frame, 1x roof cowl. For the length of the roof outlet duct and roof outlet sleeve, refer to the installation instructions.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 DFHK |
| Material: | Synthetic material |
| Colour: | grey |
| Weight: | 2,83 kg |
| Weight including packaging: | 3 kg |
| Connection diameter: | 160 mm |
| Length: | 1.180 mm |
| Width: | 160 mm |
| Height: | 160 mm |
| Depth: | 1.180 mm |
| Width with packaging: | 165 mm |
| Height with packaging: | 165 mm |
| Depth with packaging: | 1.190 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799598688 |
| Article number: | 0059.0868 |

Manufacturer: MAICO

PP 45 DFHK Roof outlet sleeve