**Roof cover frame PP 45 DER 25-35**

Roof cover frame for PP 45 roof outlet, which is installed in pitched roof.

Scope of delivery: Roof cover frame with bitumen flashing tape, grooved sealing strips, mounting material including horizontal attachment with cover pins.

A roof outlet kit comprising 1-2 roof outlet ducts, 1x short or long roof outlet sleeve, 1x roof cover frame, 1x roof cowl. For the length of the roof outlet duct and roof outlet sleeve, refer to the installation instructions.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 DER 25-35 |
| Material: | Titanium zinc |
| Colour: | Titanium zinc |
| Weight: | 6,62 kg |
| Weight including packaging: | 17,62 kg |
| Roof incline: | 25 ° - 35 ° |
| Width: | 900 mm |
| Height: | 151 mm |
| Depth: | 1.600 mm |
| Width with packaging: | 901 mm |
| Height with packaging: | 295 mm |
| Depth with packaging: | 1.601 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799991816 |
| Article number: | 0093.1316 |

Manufacturer: MAICO

PP 45 DER 25-35 Roof cover frame