**Roof cowl PP 45 DH 31-35**

Roof cowl for PP 45 roof outlet, which is installed in pitched roofs.

A roof outlet kit comprising 1-2 roof outlet ducts, 1x short or long roof outlet sleeve, 1x roof cover frame, 1x roof cowl. For the length of the roof outlet duct and roof outlet sleeve, refer to the installation instructions.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 DH 31-35 |
| Material: | Titanium zinc |
| Colour: | Titanium zinc |
| Weight: | 3,22 kg |
| Weight including packaging: | 14,22 kg |
| Roof incline: | 31 ° - 35 ° |
| Width: | 360 mm |
| Height: | 350 mm |
| Depth: | 670 mm |
| Width with packaging: | 494 mm |
| Height with packaging: | 1.200 mm |
| Depth with packaging: | 800 mm |
| Packing unit: | 1 piece |
| Suitable for products: | PP 45 DER 25-35 |
| Range: | K |
| GTIN (EAN): | 4012799991847 |
| Article number: | 0093.1319 |

Manufacturer: MAICO

PP 45 DH 31-35 Roof cowl