**Sound-absorbing element ER-SE AP**

Serves as a sound absorber and reduces the noise emissions.

ER-SE UP: for retrofitting all ER units.

ER-SE AP: for retrofitting for all ER-AP and ER-APB units.

Simple to install.

Construction material class B1.

Technical data

|  |  |
| --- | --- |
| Article: | ER-SE AP |
| Installation site: | Housing |
| Type of installation: | Surface-mounted |
| Material: | Melamine resin foam |
| Colour: | grey |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,18 kg |
| Width: | 220 mm |
| Height: | 220 mm |
| Depth: | 40 mm |
| Width with packaging: | 260 mm |
| Height with packaging: | 260 mm |
| Depth with packaging: | 90 mm |
| Total insertion loss: | 1,5 dB |
| Insertion loss note: | max. 3.5 dB |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799926795 |
| Article number: | 0192.0679 |

Manufacturer: MAICO

ER-SE AP Sound-absorbing element