**Door ventilation grille MLK 30 white**

Door ventilation grille for bathroom, WC, kitchen.

Free cross-section according to FeuVo 80 and TRGI 86.

MLK 30: Door cut-out: 271 x 111 mm, external dimension: 290 x 125 mm.

MLK 45: Door cut-out: 432 x 76 mm, external dimension: 457 x 92 mm.

Technical data

|  |  |
| --- | --- |
| Article: | MLK 30 white |
| Air direction: | Ventilation and air extraction |
| Installation: | Inside |
| Installation site: | Door |
| Material: | Synthetic material |
| Synthetic material definition: | PVC-free polystyrene |
| Colour: | White |
| Weight: | 0,2 kg |
| Weight including packaging: | 0,22 kg |
| Open cross section: | 164 cm² |
| Width: | 290 mm |
| Height: | 125 mm |
| Depth: | 38 mm |
| Width with packaging: | 300 mm |
| Height with packaging: | 125 mm |
| Depth with packaging: | 51 mm |
| Minimum door leaf thickness: | 36 mm |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799511236 |
| Article number: | 0151.0123 |

Manufacturer: MAICO

MLK 30 white Door ventilation grille