**Speed controller STX 4**

Speed controller for continuously variable control of the fans.

Minimum speed can be set.

Can be used for surface mounting and recess mounting, exception: STX 4 only for surface mounting.

Principle of function: Phase angle control.

Recommended distance from radios and TVs: 3 m.

The fans are switched on at maximum speed by turning the control knob. Turning any further reduces the speed.

Splash water protected.

Integrated temperature cut-off protection.

Orange LED operating indicator.

CE symbol.

Including spare fuse.

Additional switching contact (230 V) e.g. for controlling a shutter.

There can be a physically induced humming noise at lower speeds, through the use of phase angle technology. TRE... 5-step transformers are therefore used for speed control in rooms requiring quiet fan operations.

Mounting on walls possible, avoid ceilings as temperature builds up here.

STX 1.5, STX 2.5:

Width x height x depth when used for surface mounting: 82 mm x 89 mm x 65 mm

Width x height x depth when used for recess mounting: 50 mm x 50 mm x 35 mm

STX 4:

Width x height x depth when used for surface mounting: 82 mm x 89 mm x 65 mm

Technical data

|  |  |
| --- | --- |
| Article: | STX 4 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Maximum load: | 4 A |
| Minimum load: | 0,4 A |
| Degree of protection: | IP 44 |
| Type of installation: | Surface-mounted |
| Colour: | White, similar to RAL 9010 |
| Weight: | 0,23 kg |
| Weight including packaging: | 0,26 kg |
| Width: | 82 mm |
| Height: | 89 mm |
| Depth: | 65 mm |
| Width with packaging: | 85 mm |
| Height with packaging: | 95 mm |
| Depth with packaging: | 70 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799992288 |
| Article number: | 0157.1563 |

Manufacturer: MAICO

STX 4 Speed controller