**Speed controller, distribution board STSX 2,5**

Speed controller for continuously variable control of the fans.

VDE-tested.

For one direction of rotation.

Installation on 35 mm standard profile rail possible.

Green LED operating indicator.

There can be a physically induced humming noise at lower speeds, through the use of phase angle technology. TRE... 5-step transformers are therefore used for speed control in rooms requiring quiet fan operations.

Technical data

|  |  |
| --- | --- |
| Article: | STSX 2,5 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Maximum load: | 2,5 A |
| Minimum load: | 0,1 A |
| Degree of protection: | IP 30 |
| Type of installation: | Distributor board / control cabinet |
| Colour: | Light grey, similar to RAL 7035 |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,12 kg |
| Width: | 35 mm |
| Height: | 94 mm |
| Depth: | 86 mm |
| Width with packaging: | 40 mm |
| Height with packaging: | 95 mm |
| Depth with packaging: | 96 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799992295 |
| Article number: | 0157.1564 |

Manufacturer: MAICO

STSX 2,5 Speed controller, distribution board