**Mounting support ER-UPM**

Mounting support for installation of ER GH and ER GH-VWR flush-mounted housing on walls, ceilings or in shafts.

With 2 different slots (5mm / 8mm) for accurately adjusting the fan housing using a hammer head screw or mounting screws.

Packing unit:

2 L-shaped angle plates

4 mounting screws.

Technical data

|  |  |
| --- | --- |
| Article: | ER-UPM |
| Material: | Sheet steel, galvanised |
| Weight: | 0,4 kg |
| Weight including packaging: | 0,45 kg |
| Width: | 350 mm |
| Height: | 40 mm |
| Depth: | 50 mm |
| Width with packaging: | 351 mm |
| Height with packaging: | 46 mm |
| Depth with packaging: | 56 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799932772 |
| Article number: | 0093.0277 |

Manufacturer: MAICO

ER-UPM Mounting support