**Air filter, replacement ZF ECD+**

ZF ECD+ replacement continuous air filter for the ER-A covers of the ER EC fan insert.

With time strip as filter change indicator.

Can be washed under warm water.

Technical data

|  |  |
| --- | --- |
| Article: | ZF ECD+ |
| Installation position: | vertical / horizontal |
| Weight: | 0,02 kg |
| Weight including packaging: | 0,03 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Width: | 135 mm |
| Height: | 135 mm |
| Depth: | 8 mm |
| Width with packaging: | 255 mm |
| Height with packaging: | 175 mm |
| Depth with packaging: | 20 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 2 pieces |
| Range: | B |
| GTIN (EAN): | 4012799992325 |
| Article number: | 0093.1562 |

Manufacturer: MAICO

ZF ECD+ Air filter, replacement