**PREHEATING REGISTER WS-VH 300**

Electric PTC preheating register for continuous operation of the WS 300 Flat centralised ventilation units at very low outside temperatures.

Technical data

|  |  |
| --- | --- |
| Article: | WS-VH 300 |
| Rated voltage: | 230 VAC |
| Frequency: | 50 Hz |
| Degree of protection: | IP 00 |
| Weight: | 1,02 kg |
| Weight including packaging: | 1,1 kg |
| Width: | 318 mm |
| Height: | 220 mm |
| Depth: | 51 mm |
| Width with packaging: | 322 mm |
| Height with packaging: | 230 mm |
| Depth with packaging: | 60 mm |
| Heater power rating: | 1.000 W |
| Packing unit: | 1 piece |
| Suitable for products: | WS 300 Flat R, L, BR, BL |
| Range: | K |
| GTIN (EAN): | 4012799992202 |
| Article number: | 0093.1322 |

Manufacturer: MAICO

WS-VH 300 PREHEATING REGISTER