**Air filter TFE 16-4**

Air filter for ventilation systems.

Inspection lid can be removed for easy filter exchange.

With filter insert made of synthetic fibre.

Filter insert cannot be regenerated.

With rubber seal on the air connection couplings.

Accessories: Replacement air filter FE.. .

Recommended accessories: DW 1000 differential pressure controller.

Installation instructions

Monitor filter resistance using DW 1000 differential pressure controller.

Technical data

|  |  |
| --- | --- |
| Article: | TFE 16-4 |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 2,6 kg |
| Weight including packaging: | 2,97 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Nominal size: | 160 mm |
| Width: | 260 mm |
| Height: | 230 mm |
| Depth: | 205 mm |
| Width with packaging: | 290 mm |
| Height with packaging: | 300 mm |
| Depth with packaging: | 260 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490777 |
| Article number: | 0149.0077 |

Manufacturer: MAICO

TFE 16-4 Air filter