**Air filter TFE 20-4**

Air filter for ventilation systems.

Inspection lid can be removed for easy filter exchange.

With filter insert made of synthetic fibre.

Filter insert cannot be regenerated.

With rubber seal on the air connection couplings.

Accessories: Replacement air filter FE.. .

Recommended accessories: DW 1000 differential pressure controller.

Installation instructions

Monitor filter resistance using DW 1000 differential pressure controller.

Technical data

|  |  |
| --- | --- |
| Article: | TFE 20-4 |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 3,45 kg |
| Weight including packaging: | 3,78 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Nominal size: | 200 mm |
| Width: | 310 mm |
| Height: | 275 mm |
| Depth: | 230 mm |
| Width with packaging: | 350 mm |
| Height with packaging: | 320 mm |
| Depth with packaging: | 300 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490784 |
| Article number: | 0149.0078 |

Manufacturer: MAICO

TFE 20-4 Air filter