**Air filter TFE 25-4**

Air filter for ventilation systems.

Inspection lid can be removed for easy filter exchange.

With filter insert made of synthetic fibre.

Filter insert cannot be regenerated.

With rubber seal on the air connection couplings.

Accessories: Replacement air filter FE.. .

Recommended accessories: DW 1000 differential pressure controller.

Technical data

|  |  |
| --- | --- |
| Article: | TFE 25-4 |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 5,05 kg |
| Weight including packaging: | 5,63 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Nominal size: | 250 mm |
| Width: | 365 mm |
| Height: | 325 mm |
| Depth: | 325 mm |
| Width with packaging: | 400 mm |
| Height with packaging: | 380 mm |
| Depth with packaging: | 350 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490791 |
| Article number: | 0149.0079 |

Manufacturer: MAICO

TFE 25-4 Air filter