**Air filter TFE 31-4**

Air filter for ventilation systems.

Inspection lid can be removed for easy filter exchange.

With filter insert made of synthetic fibre.

Filter insert cannot be regenerated.

With rubber seal on the air connection couplings.

Accessories: Replacement air filter FE.. .

Recommended accessories: DW 1000 differential pressure controller.

Installation instructions

Monitor filter resistance using DW 1000 differential pressure controller.

Technical data

|  |  |
| --- | --- |
| Article: | TFE 31-4 |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 7,41 kg |
| Weight including packaging: | 8,03 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Nominal size: | 315 mm |
| Width: | 425 mm |
| Height: | 390 mm |
| Depth: | 420 mm |
| Width with packaging: | 465 mm |
| Height with packaging: | 405 mm |
| Depth with packaging: | 470 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490807 |
| Article number: | 0149.0080 |

Manufacturer: MAICO

TFE 31-4 Air filter