**Air distributor made of plastic, 8-way MF-V63**

Air distributor with several connections for MF-F flexible ducts.

Made from sound-proof material.

With revision opening.

Revision opening either to the side of or on the underside of the distributor.

With pre-drilled holes for installation with threaded rods.

Long working life and environmental stability.

Technical data

|  |  |
| --- | --- |
| Article: | MF-V63 |
| Air direction: | Ventilation and air extraction |
| Volumetric flow: | 160 m³/h recommended |
| Installation site: | Ceiling / Wall / Floor |
| Material: | Plastic EPP |
| Synthetic material definition: | PVC-free |
| Weight: | 0,86 kg |
| Weight including packaging: | 0,9 kg |
| Connection diameter: | 125 mm |
| Flexible steel duct connection diameter: | 63 mm |
| Number of couplings: | 8 |
| Width: | 435 mm |
| Height: | 150 mm |
| Depth: | 270 mm |
| Width with packaging: | 435 mm |
| Height with packaging: | 150 mm |
| Depth with packaging: | 270 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799599708 |
| Article number: | 0059.0970 |

Manufacturer: MAICO

MF-V63 Air distributor made of plastic, 8-way