**Bracket MF-WL125 80/200**

90° adaptor for round cross-section (supply air or exhaust air valve) on MF-WE slide-in adaptor.

Connection couplings with collar size.

Technical data

|  |  |
| --- | --- |
| Article: | MF-WL125 80/200 |
| Air direction: | Ventilation and air extraction |
| Installation site: | Ceiling / Floor / Wall |
| Material: | Sheet steel, galvanised |
| Weight: | 1,15 kg |
| Weight including packaging: | 1,2 kg |
| Nominal size: | 125 mm |
| Width: | 277,5 mm |
| Height: | 390 mm |
| Depth: | 200 mm |
| Width with packaging: | 277,5 mm |
| Height with packaging: | 390 mm |
| Depth with packaging: | 200 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799185314 |
| Article number: | 0018.0531 |

Manufacturer: MAICO

MF-WL125 80/200 Bracket