**Air filter, replacement WSF 300-400**

Replacement air filter for WR 300 or WR 400 centralised ventilation units.

Technical data

|  |  |
| --- | --- |
| Article: | WSF 300-400 |
| Installation position: | vertical / horizontal |
| Weight: | 0,31 kg |
| Weight including packaging: | 0,46 kg |
| Filter class: | ISO Coarse 80 % (G4) / ISO ePM1 55 % (F7) |
| Width: | 425 mm |
| Height: | 175 mm |
| Depth: | 48 mm |
| Width with packaging: | 500 mm |
| Height with packaging: | 195 mm |
| Depth with packaging: | 80 mm |
| Packing unit: | 1 set (3 pieces) |
| Suitable for products: | WR 300, WR 400 |
| Range: | K |
| GTIN (EAN): | 4012799938989 |
| Article number: | 0093.0898 |

Manufacturer: MAICO

WSF 300-400 Air filter, replacement