**Small room fan ECA 11-1 K**

Technical data

|  |  |
| --- | --- |
| Article: | ECA 11-1 K |
| Model: | Standard model |
| Air flow volume: | 95 m³/h |
| Rotating speed: | 2.650 1/min |
| Air direction: | Air extraction |
| Speed controllable: | ✔ |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Power consumption: | 13 W |
| Imax: | 0,1 A |
| Degree of protection: | IP 44 |
| Installation site: | Ceiling / Wall |
| Installation position: | any |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,75 |
| Nominal size: | 100 mm |
| Packing unit: | 1 piece |
| Article number: | 0080.0504 |

Manufacturer: MAICO

ECA 11-1 K Small room fan