**Surface-mounted fan ERA 11**

Technical data

|  |  |
| --- | --- |
| Article: | ERA 11 |
| Air flow volume: | 70 m³/h / 110 m³/h |
| Rotating speed: | 1.620 1/min / 2.410 1/min |
| Power consumption: | 28 W / 35 W |
| Imax: | 0,14 A / 0,16 A |
| Degree of protection: | IP 54 |
| Weight: | 1,3 |
| Pulley integrated: | - |
| Packing unit: | 1 piece |
| Article number: | 0080.0105 |

Manufacturer: MAICO

ERA 11 Surface-mounted fan