**5-step transformer TRE 1,6-1**

5-step transformers for setting speed.

To control AC fans.

With operating indicator light.

Additional switching contact (230 V) e.g. for controlling a shutter.

Technical data

|  |  |
| --- | --- |
| Article: | TRE 1,6-1 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 1,6 A |
| Degree of protection: | IP 54 |
| Type of installation: | Surface-mounted |
| Housing material: | Synthetic material |
| Colour: | Light grey, similar to RAL 7035 |
| Weight: | 1,6 kg |
| Weight including packaging: | 1,8 kg |
| Width: | 193 mm |
| Height: | 123 mm |
| Depth: | 105 mm |
| Width with packaging: | 200 mm |
| Height with packaging: | 185 mm |
| Depth with packaging: | 150 mm |
| Ambient temperature: | 0 °C up to 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799573487 |
| Article number: | 0157.0348 |

Manufacturer: MAICO

TRE 1,6-1 5-step transformer