**Axial roof fan DZD 30/84 A**

Technical data

|  |  |
| --- | --- |
| Article: | DZD 30/84 A |
| Air flow volume: | 580 m³/h / 1.500 m³/h |
| Rotating speed: | 715 1/min / 1.425 1/min |
| Power consumption: | 33 W / 105 W |
| Imax: | 0,1 A / 0,28 A |
| Degree of protection: | IP 55 |
| Pole-changeable: | ✔ |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 15 |
| Packing unit: | 1 piece |
| Article number: | 0087.0434 |

Manufacturer: MAICO

DZD 30/84 A Axial roof fan