**Axial roof fan DZD 40/42 A**

Technical data

|  |  |
| --- | --- |
| Article: | DZD 40/42 A |
| Air flow volume: | 3.200 m³/h / 7.300 m³/h |
| Rotating speed: | 1.425 1/min / 2.850 1/min |
| Power consumption: | 260 W / 1.600 W |
| Imax: | 0,9 A / 3 A |
| Degree of protection: | IP 55 |
| Pole-changeable: | ✔ |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 36,8 |
| Packing unit: | 1 piece |
| Article number: | 0087.0446 |

Manufacturer: MAICO

DZD 40/42 A Axial roof fan