**Axial roof fan DZD 35/2 A**

Technical data

|  |  |
| --- | --- |
| Article: | DZD 35/2 A |
| Air flow volume: | 4.450 m³/h |
| Rotating speed: | 2.850 1/min |
| Power consumption: | 860 W |
| Imax: | 1,9 A |
| Degree of protection: | IP 55 |
| Pole-changeable: |  -  |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 26 |
| Packing unit: | 1 piece |
| Article number: | 0087.0419 |

Manufacturer: MAICO

DZD 35/2 A Axial roof fan