**Axial roof fan EZD 40/6 A**

Technical data

|  |  |
| --- | --- |
| Article: | EZD 40/6 A |
| Air flow volume: | 2.050 m³/h |
| Rotating speed: | 930 1/min |
| Power consumption: | 100 W |
| Imax: | 0,5 A |
| Degree of protection: | IP 55 |
| Pole-changeable: | - |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 23 |
| Packing unit: | 1 piece |
| Article number: | 0087.0408 |

Manufacturer: MAICO

EZD 40/6 A Axial roof fan