**Outside air opening ALD 10**

Outside air opening for draught-free, decentralised domestic ventilation.

Linear control of the air flow.

No electrical connection required.

Packing unit: Internal part, dust or insect filter, wall sleeve up to 500 mm, external grille with fly screen.

Accessories: ALDS 10 storm protection, ALDF 10 replacement filter.

Technical data

|  |  |
| --- | --- |
| Article: | ALD 10 |
| Air direction: | Ventilation |
| Max. volumetric flow: | 32 m³/h / at 10 Pa |
| Installation site: | Wall |
| Material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,98 kg |
| Weight including packaging: | 1,21 kg |
| Type of filter: | Dust filter |
| Filter class: | ISO Coarse 30 % (G2) |
| Type of shutter: | manual |
| Nominal size: | 100 mm |
| Width: | 150 mm |
| Height: | 150 mm |
| Depth: | 580 mm |
| Width with packaging: | 280 mm |
| Height with packaging: | 155 mm |
| Depth with packaging: | 280 mm |
| Ambient temperature: | 60 °C |
| Rated max. element normal difference in noise level Dn,w: | 31 dB |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799520542 |
| Article number: | 0152.0054 |

Manufacturer: MAICO

ALD 10 Outside air opening