**Disk valve, metal TFZ 12**

Disk valve for ventilation.

Attractive, flat model.

Linear air flow control via rotatable valve disk.

With bayonet closure for mounting frame.

Accessories needed: Mounting frame with EBR-D / EBR sealing.

Technical data

|  |  |
| --- | --- |
| Article: | TFZ 12 |
| Air direction: | Ventilation |
| Max. volumetric flow: | 60 m³/h |
| Material: | Sheet steel, galvanised |
| Colour: | Pure white, similar to RAL 9010, gloss 70 |
| Weight: | 0,29 kg |
| Weight including packaging: | 0,3 kg |
| Suitable for nominal size: | 125 mm |
| Width: | 160 mm |
| Height: | 160 mm |
| Depth: | 163 mm |
| Width with packaging: | 163 mm |
| Height with packaging: | 68 mm |
| Depth with packaging: | 163 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799513650 |
| Article number: | 0151.0365 |

Manufacturer: MAICO

TFZ 12 Disk valve, metal