**Disk valve, stainless steel TM-V2A 10**

Stainless steel disk valves for ventilation and air extraction with connection socket.

With loose installation ring and spring clamp for simple installation.

Linear air flow control via rotatable valve disk.

Recommended accessories: FFE grease filter element for use in rooms where the exhaust air contains grease (e.g. kitchens etc.).

Technical data

|  |  |
| --- | --- |
| Article: | TM-V2A 10 |
| Air direction: | Ventilation and air extraction |
| Volumetric flow: | 30 m³/h / 40 m³/h / 60 m³/h / 80 m³/h at 15 Pa / 25 Pa / 53 Pa / 100 Pa |
| Material: | Stainless steel |
| Colour: | Stainless steel, brushed |
| Weight: | 0,2 kg |
| Weight including packaging: | 0,21 kg |
| Suitable for nominal size: | 100 mm |
| Width: | 140 mm |
| Height: | 140 mm |
| Depth: | 52 mm |
| Width with packaging: | 141 mm |
| Height with packaging: | 141 mm |
| Depth with packaging: | 60 mm |
| Sound power level: | 35 dB(A) / at max. 80 m³/h |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799513742 |
| Article number: | 0151.0374 |

Manufacturer: MAICO

TM-V2A 10 Disk valve, stainless steel