**Timer ZS 4**

Two-channel timer for installation in distributor.

Can be programmed without mains connection (6 years of power reserve).

Text-based menu guidance and self-explanatory icons/symbols.

Large and clear display with two high-resolution rows of text (matrix of dots).

Easy to use. Quick and intuitive to program.

46 memory spaces.

Day and week program.

Holiday and impulse program.

Permanent switching by date.

Manual permanent switching.

Manual switching forestalling.

Automatic switching time orientation when reading.

Automatic summer time setting.

Display of device operating hours and per channel.

Security by means of PIN coding.

2 changeover contacts.

Shortest switching spacing of 1 min.

Switching capacity 16 A / 250 V.

Technical data

|  |  |
| --- | --- |
| Article: | ZS 4 |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Power consumption: | 1,5 W |
| Degree of protection: | IP 20 |
| Electrical plug-type connection: | Screw connection |
| Type of installation: | Distribution board |
| Housing material: | Synthetic material |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,17 kg |
| Width: | 36 mm |
| Height: | 90 mm |
| Depth: | 58 mm |
| Width with packaging: | 40 mm |
| Height with packaging: | 110 mm |
| Depth with packaging: | 67 mm |
| Ambient temperature: | -10 °C up to 50 °C |
| Remote control: |  -  |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799570882 |
| Article number: | 0157.0088 |

Manufacturer: MAICO

ZS 4 Timer