**Air distributor made of plastic, 8-way MF-V75-8**

Air distributor with 8 connections for MF-F flexible ducts.

Made from sound-proof material.

Optimum air distribution thanks to integrated balanced-flow conductors.

With 2 inspection openings on sides.

With pre-drilled holes for installation with threaded rods.

Long working life and environmental stability.

Technical data

|  |  |
| --- | --- |
| Article: | MF-V75-8 |
| Air direction: | Ventilation and air extraction |
| Volumetric flow: | 300 m³/h recommended |
| Installation site: | Ceiling / Wall / Floor |
| Material: | Plastic EPP |
| Synthetic material definition: | PVC-free |
| Weight: | 1,85 kg |
| Weight including packaging: | 1,9 kg |
| Connection diameter: | 160 mm |
| Flexible steel duct connection diameter: | 75 mm |
| Number of couplings: | 8 |
| Width: | 710 mm |
| Height: | 185 mm |
| Depth: | 350 mm |
| Width with packaging: | 712 mm |
| Height with packaging: | 187 mm |
| Depth with packaging: | 380 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799599807 |
| Article number: | 0059.0980 |

Manufacturer: MAICO

MF-V75-8 Air distributor made of plastic, 8-way