**Slide-in sound absorber SDE 8**

Can be used as sound absorber or for pressure control in flexible and folded spiral-seams ducts.

Suitable for ventilation and air extraction.

Can be adjusted to the given circumstances by removing plugs.

Small hole intended for measuring the air volumes.

Low space requirement.

Simple to install.

Can be retro-fitted.

Fire- and mould-proof foam, compliant with emission class M1 requirements.

Easy to clean with a vacuum cleaner.

Technical data

|  |  |
| --- | --- |
| Article: | SDE 8 |
| Installation site: | Duct |
| Material: | PU foam |
| Weight: | 0,03 kg |
| Weight including packaging: | 0,03 kg |
| Nominal size: | 80 mm |
| Suitable for nominal size: | 80 |
| External diameter: | 82 mm |
| Width: | 80 mm |
| Height: | 60 mm |
| Depth: | 50 mm |
| Width with packaging: | 81 mm |
| Height with packaging: | 61 mm |
| Depth with packaging: | 51 mm |
| Insertion loss at 125 Hz: | 9 dB / 4,5 dB / 4,5 dB |
| Insertion loss at 250 Hz: | 5 dB / 3,5 dB / 2,5 dB |
| Insertion loss at 500 Hz: | 11,5 dB / 7,5 dB / 5 dB |
| Insertion loss at 1 kHz: | 14,5 dB / 11,5 dB / 8 dB |
| Insertion loss at 2 kHz: | 18 dB / 10,5 dB / 9,5 dB |
| Insertion loss at 4 kHz: | 20 dB / 17,5 dB / 13 dB |
| Insertion loss at 8 kHz: | 24 dB / 21 dB / 15,5 dB |
| Insertion loss note: | indications for 1, 3 and 5 openings |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799442134 |
| Article number: | 0044.0213 |

Manufacturer: Jeven

SDE 8 Slide-in sound absorber