**Slide-in sound absorber SDE 10**

Can be used as sound absorber or for pressure control in flexible and folded spiral-seams ducts.

Suitable for ventilation and air extraction.

Can be adjusted to the given circumstances by removing plugs.

Small hole intended for measuring the air volumes.

Low space requirement.

Simple to install.

Can be retro-fitted.

Fire- and mould-proof foam, compliant with emission class M1 requirements.

Easy to clean with a vacuum cleaner.

Technical data

|  |  |
| --- | --- |
| Article: | SDE 10 |
| Installation site: | Duct |
| Material: | PU foam |
| Weight: | 0,06 kg |
| Weight including packaging: | 0,1 kg |
| Nominal size: | 100 mm |
| Suitable for nominal size: | 100 |
| External diameter: | 102 mm |
| Width: | 100 mm |
| Height: | 100 mm |
| Depth: | 50 mm |
| Width with packaging: | 100 mm |
| Height with packaging: | 100 mm |
| Depth with packaging: | 50 mm |
| Insertion loss at 63 Hz: | 6,5 dB / 3 dB / 1,5 dB |
| Insertion loss at 125 Hz: | 7 dB / 3,5 dB / 2,5 dB |
| Insertion loss at 250 Hz: | 4 dB / 2,5 dB / 1,5 dB |
| Insertion loss at 500 Hz: | 9,5 dB / 5,5 dB / 3,5 dB |
| Insertion loss at 1 kHz: | 13 dB / 8,5 dB / 6 dB |
| Insertion loss at 2 kHz: | 16 dB / 8,5 dB / 6,5 dB |
| Insertion loss at 4 kHz: | 18 dB / 15 dB / 12 dB |
| Insertion loss at 8 kHz: | 22 dB / 19 dB / 17 dB |
| Insertion loss note: | indications for 1, 3 and 5 openings |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799442141 |
| Article number: | 0044.0214 |

Manufacturer: Jeven

SDE 10 Slide-in sound absorber