**Supply air valve ZWVQ 10**

In an attractive design for installation on the wall with horizontal air exit. High induction effect with the room air provides good air mixing and draught-free air supply, even at lower temperatures.

The large range offered by the valve enables a high inflow depth.

Installation close to the ceiling possible.

Thanks to its smooth front panel, the supply air valve is very easy to keep clean.

Removable front panel.

A simple and accurate volumetric flow setting can be achieved by removing or adding the supplied, invisible stick-on strips over the rows of holes.

Low background noise.

The valve with duct connection and rubber seal can be pushed straight into the folded spiral-seams duct.

Technical data

|  |  |
| --- | --- |
| Article: | ZWVQ 10 |
| Air direction: | Ventilation |
| Max. volumetric flow: | 50 m³/h |
| Installation: | Inside |
| Installation site: | Wall |
| Material: | Sheet steel, galvanised |
| Colour: | White powder-coated, similar to RAL 9010 |
| Weight: | 0,67 kg |
| Weight including packaging: | 0,69 kg |
| Nominal size: | 100 mm |
| Width: | 218 mm |
| Height: | 156 mm |
| Depth: | 60 mm |
| Width with packaging: | 220 mm |
| Height with packaging: | 160 mm |
| Depth with packaging: | 90 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799520641 |
| Article number: | 0152.0064 |

Manufacturer: MAICO

ZWVQ 10 Supply air valve