**Recessed-mounted housing ER - UP/G**

Single-room air extraction

Flush-mounted housing for fitting an ER 60 ... or ER 100 ... fan.

Installation in bathrooms, WCs and open-plan kitchens.

Plastic exhaust socket with airstream-operated plastic backflow preventer.

Plastic backflow preventer also serves as a cold smoke preventer.

DN 75/80 connection diameter.

Easily removable backflow preventer, thus simple and quick cleaning.

Installation inside and outside the wall and ceiling shafts is possible.

Reduced overall depth of the flush-mounted housing and the cover.

Permitted for an air outlet direction upward, to the right or left.

With plaster protective cover.

Practical snap-on-attachment and electrical plug connector for quick fan installation in the housing.

Knockout points in the housing for using the ER-AS extraction socket for toilet seat air extraction.

Plastic parts are normally inflammable in accordance with class B 2.

National technical approval, approval no.: Z-51.1-7;

Certificates of approval on request or on our website – www.maico-ventilatoren.com.

Second room air extraction

ER-ZR second room connection kit for second room air extraction.

Knockout points for the additional connection socket on the right, left and lower side have been fitted in the ER-UP/G housing.

Fan types which can be used for second room air extraction in accordance with DIN 18017-3: ER 100, ER 100 VZ, ER 100 VZ 15, ER 100 VZC, ER 100 G, ER 100 I, ER 100 D or ER 100 RC.

Main room: 60 m3/h

Second room: 40 m3/h

Technical data

|  |  |
| --- | --- |
| Article: | ER - UP/G |
| Model: | Plastic exhaust socket at side with airstream-operated plastic backflow preventer, without fire protection housing, second room connection possible on right/left/at bottom |
| Air direction: | Air extraction |
| Installation site: | Wall / Ceiling |
| Type of installation: | Recessed-mounted |
| Material: | Synthetic material |
| Colour: | Black |
| Weight: | 0,48 kg |
| Weight including packaging: | 0,74 kg |
| Fire protection: | No |
| Air outlet direction: | at side |
| Connection diameter: | 75 mm / 80 mm |
| Width: | 225 mm |
| Height: | 225 mm |
| Depth: | 108 mm |
| Width with packaging: | 320 mm |
| Height with packaging: | 240 mm |
| Depth with packaging: | 130 mm |
| Approval number: | Z-51.1-7 |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799939955 |
| Article number: | 0093.0995 |

Manufacturer: MAICO

ER - UP/G Recessed-mounted housing