**Recessed-mounted housing ER - UPD**

Single-room air extraction

Flush-mounted housing for fitting an ER 60 ... or ER 100 ... fan.

Installation in open-plan kitchens, bathrooms and WCs.

With K90-18017 maintenance-free fire protection shut-off device against spread of fire.

DN 75/80 metal exhaust socket with metal shut-off damper and airstream-operated release mechanism.

Metal shut-off damper also serves as a cold smoke preventer.

Easily removable backflow preventer, thus simple and quick cleaning.

Installation inside and outside the wall and ceiling shafts is possible.

Permitted for an air outlet direction upward, to the right or left.

Reduced overall depth of the flush-mounted housing and the cover.

With plaster protective cover.

Practical snap-on-attachment and electrical plug connector for quick fan installation in the housing.

Knockout points in the housing for using the ER-AS extraction socket for toilet seat air extraction.

Plastic parts are normally inflammable in accordance with class B 2.

National technical approval, approval no.: Z-51.1-46;

Certificates of approval on request or on our website – www.maico-ventilatoren.com.

Second room air extraction

ER-ZR second room connection kit for second room air extraction.

Knockout points for the additional connection socket on the right, left and lower side have been fitted in the ER-UPD housing.

Fan types which can be used for second room ventilation in accordance with DIN 18017-3: ER 100, ER 100 VZ, ER 100 VZ 15, ER 100 VZC, ER 100 G, ER 100 I, ER 100 D or ER 100 RC.

Main room: 60 m3/h

Second room: 40 m3/h

Technical data

|  |  |
| --- | --- |
| Article: | ER - UPD |
| Model: | Metal exhaust socket at side with metal shut-off shutter, with airstream-operated triggering device, without fire protection housing, second room connection possible on right/left/at bottom |
| Air direction: | Air extraction |
| Installation site: | Wall / Ceiling |
| Type of installation: | Recessed-mounted |
| Material: | Synthetic material |
| Colour: | Black |
| Weight: | 0,66 kg |
| Weight including packaging: | 0,93 kg |
| Fire protection: | yes |
| Shut-off device: | integrated |
| Air outlet direction: | at side |
| Connection diameter: | 75 mm / 80 mm |
| Width: | 225 mm |
| Height: | 225 mm |
| Depth: | 108 mm |
| Width with packaging: | 310 mm |
| Height with packaging: | 240 mm |
| Depth with packaging: | 120 mm |
| Approval number: | Z-51.1-46 |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799939726 |
| Article number: | 0093.0972 |

Manufacturer: MAICO

ER - UPD Recessed-mounted housing