**Recessed-mounted housing ER - UPB/U**

Single-room air extraction

Fire protection housing for fitting an ER 60 ... or ER 100 ... fan.

Installation in open-plan kitchens, bathrooms and WCs.

With K90-18017 maintenance-free fire protection shut-off device against spread of fire.

DN 75/80 metal exhaust socket with metal shut-off damper and airstream-operated release mechanism.

Metal shut-off damper also serves as a cold smoke preventer.

Easily removable backflow preventer, thus simple and quick cleaning.

Installation inside the wall and ceiling shafts is possible.

Approved for wall installation with air outlet direction upwards, right or left, as well as ceiling installation.

Reduced overall depth of the flush-mounted housing and the cover.

With plaster protective cover.

Practical snap-on-attachment and electrical plug connector for quick fan installation in the housing.

Plastic parts are normally inflammable in accordance with class B 2.

National technical approval, approval no.: Z-51.1-46;

Certificates of approval on request or on our website – www.maico-ventilatoren.com.

Second room air extraction

ER-UPB housings with integrated second room connection kit can be supplied for second room air extraction:

UPB/R : right.

UPB/L : left.

UPB/U : bottom.

Fan types which can be used for second room ventilation in accordance with DIN 18017-3: ER 100, ER 100 VZ, ER 100 VZ 15, ER 100 VZC, ER 100 G, ER 100 I, ER 100 D or ER 100 RC.

Main room: 60 m3/h

Second room: 40 m3/h

Technical data

|  |  |
| --- | --- |
| Article: | ER - UPB/U |
| Model: | Metal exhaust socket at side with metal shut-off shutter, with airstream-operated triggering device, with fire protection housing, second room connection at bottom |
| Air direction: | Air extraction |
| Installation site: | Wall / Ceiling |
| Type of installation: | Recessed-mounted |
| Material: | Synthetic material |
| Colour: | Black |
| Weight: | 2,52 kg |
| Weight including packaging: | 3,01 kg |
| Fire protection: | yes |
| Shut-off device: | integrated |
| Air outlet direction: | at side |
| Connection diameter: | 75 mm / 80 mm |
| Width: | 249 mm |
| Height: | 249 mm |
| Depth: | 120 mm |
| Width with packaging: | 415 mm |
| Height with packaging: | 280 mm |
| Depth with packaging: | 130 mm |
| Approval number: | Z-51.1-46 |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799939719 |
| Article number: | 0093.0971 |

Manufacturer: MAICO

ER - UPB/U Recessed-mounted housing