**Axial roof fan DZD 40/8 A**

Technical data

|  |  |
| --- | --- |
| Article: | DZD 40/8 A |
| Air flow volume: | 1.600 m³/h |
| Rotating speed: | 715 1/min |
| Power consumption: | 75 W |
| Imax: | 0,2 A |
| Degree of protection: | IP 55 |
| Pole-changeable: |  -  |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 21,8 |
| Packing unit: | 1 piece |
| Article number: | 0087.0420 |

Manufacturer: MAICO

DZD 40/8 A Axial roof fan