**ECO 40 D**

Features ECO 30 E, ECO 40 D

Oscillating fan.

Suitable for wall installation.

Minimum mounting height = 2.3 m (distance between lower impeller edge and floor).

With yellow chromated protective cage, protection against accidental contact in accordance with DIN EN ISO 13857.

3-blade impeller made of plastic.

Adjustable pivoting angle: 55°, 70°, 90° or 115°.

Fan and swivel gear drives can be switched separately.

Motor

Asynchronous motor.

Thermal overload protection as standard feature.

Mounting instructions

Individual components must be fitted on site.

Mounting hooks must be provided by the customer.

Electrical connection

To terminal blocks in the canopy's connection area.

Special versions

The following special versions are available at extra cost on request:

Special voltages and frequencies.

Information on operation at temperatures occasionally below -20 °C available upon request.

If operating with frequency converters, the factory must be consulted.

Feasibility must be checked in each case.

Technical data

|  |  |
| --- | --- |
| Article: | ECO 40 D |
| Maximum air circulation: | 4.500 m³/h |
| Rotating speed: | 1.150 1/min |
| Impeller diameter: | 400 mm |
| Impeller type: | axial |
| Speed controllable: |  ✔  |
| Reversing capacity: |  -  |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Power consumption: | 44 W |
| Imax: | 0,25 A |
| Degree of protection: | IP 20 |
| Installation site: | Wall |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material |
| Colour: | similar to pearl white, RAL 1013 |
| Weight: | 3,97 kg |
| Weight including packaging: | 4,84 kg |
| Swivellable: |  ✔  |
| Width: | 450 mm |
| Height: | 450 mm |
| Depth: | 340 mm |
| Width with packaging: | 451 mm |
| Height with packaging: | 451 mm |
| Depth with packaging: | 385 mm |
| Airstream temperature at nominal current: | 40 °C |
| Airstream temperature at IMax: | 40 °C |
| Ambient temperature: | 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799880141 |
| Article number: | 0088.0014 |

Manufacturer: MAICO

ECO 40 D