**Sound-insulated ventilation box ESR 20/1**

Technical data

|  |  |
| --- | --- |
| Article: | ESR 20/1 |
| Air flow volume: | 700 m³/h |
| Rotating speed: | 1.450 1/min |
| Speed controllable: | - |
| Nominal output: | 140 W |
| Inom: | 0,6 A |
| Imax: | 0,6 A |
| Degree of protection: | IP X4 |
| Insulation class: | B |
| Weight: | 15,3 |
| Nominal size: | 200 mm |
| Airstream temperature at nominal current: | 45 °C |
| Airstream temperature at IMax: | 45 °C Required Delta p<sub>st</sub> min = 50 Pa |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799802839 |
| Article number: | 0080.0283 |

Manufacturer: MAICO

ESR 20/1 Sound-insulated ventilation box