**Sound-insulated ventilation box ESR 40/1**

Technical data

|  |  |
| --- | --- |
| Article: | ESR 40/1 |
| Air flow volume: | 2.500 m³/h |
| Rotating speed: | 1.200 1/min |
| Speed controllable: |  -  |
| Nominal output: | 585 W |
| Inom: | 3 A |
| Imax: | 3 A |
| Degree of protection: | IP X4 |
| Insulation class: | F |
| Weight: | 40,14 |
| Weight including packaging: | 43,12 kg |
| Nominal size: | 400 mm |
| Width with packaging: | 785 mm |
| Height with packaging: | 500 mm |
| Depth with packaging: | 615 mm |
| Airstream temperature at IMax: | 50 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799802877 |
| Article number: | 0080.0287 |

Manufacturer: MAICO

ESR 40/1 Sound-insulated ventilation box