**Sound-insulated ventilation box ESR 16 S**

Technical data

|  |  |
| --- | --- |
| Article: | ESR 16 S |
| Air flow volume: | 550 m³/h |
| Rotating speed: | 2.530 1/min |
| Speed controllable: |  -  |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Nominal output: | 95 W |
| Inom: | 0,41 A |
| Imax: | 0,5 A |
| Weight: | 20 |
| Swivelling fan: |  -  |
| Nominal size: | 160 mm |
| Airstream temperature at nominal current: | 80 °C |
| Ambient temperature: | 80 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799802280 |
| Article number: | 0080.0228 |

Manufacturer: MAICO

ESR 16 S Sound-insulated ventilation box