**Sound-insulated ventilation box DSR 35 S**

Technical data

|  |  |
| --- | --- |
| Article: | DSR 35 S |
| Air flow volume: | 2.865 m³/h |
| Rotating speed: | 1.360 1/min |
| Speed controllable: | - |
| Type of voltage: | Three-phase AC |
| Rated voltage: | 400 V |
| Nominal output: | 470 W |
| Inom: | 1,18 A |
| Imax: | 1,3 A |
| Mains cable: | 5 x 1,5 mm² |
| Weight: | 46 |
| Swivelling fan: | - |
| Nominal size: | 355 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799802327 |
| Article number: | 0080.0232 |

Manufacturer: MAICO

DSR 35 S Sound-insulated ventilation box