**External grille LZP-R 22**

Weather protection grille for ventilation and air extraction constructed to very high quality standard.

With channel cross-section extension as standard to reduce pressure losses.

With fixed rain-repellent weather protection lamella.

With frame for mounting in masonry walls.

With 20 mm flange frame and slots for direct connection with channel.

Protective grille in accordance with DIN EN ISO 13857.

Technical data

|  |  |
| --- | --- |
| Article: | LZP-R 22 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Wall / Channel |
| Material: | Sheet steel, galvanised |
| Weight: | 13 kg |
| Weight including packaging: | 13,575 kg |
| Channel dimension: | 500 mm x 250 mm |
| Open cross section: | 1.012 cm² |
| Width: | 779 mm |
| Height: | 325 mm |
| Depth: | 250 mm |
| Width with packaging: | 880 mm |
| Height with packaging: | 340 mm |
| Depth with packaging: | 320 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799513810 |
| Article number: | 0151.0381 |

Manufacturer: MAICO

LZP-R 22 External grille