**External grille LZP-R 28**

Weather protection grille for ventilation and air extraction constructed to very high quality standard.

With channel cross-section extension as standard to reduce pressure losses.

With fixed rain-repellent weather protection lamella.

With frame for mounting in masonry walls.

With 20 mm flange frame and slots for direct connection with channel.

Protective grille in accordance with DIN EN ISO 13857.

Technical data

|  |  |
| --- | --- |
| Article: | LZP-R 28 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Wall / Channel |
| Material: | Sheet steel, galvanised |
| Weight: | 16,5 kg |
| Weight including packaging: | 18,23 kg |
| Channel dimension: | 600 mm x 300 mm |
| Open cross section: | 1.458 cm² |
| Width: | 929 mm |
| Height: | 375 mm |
| Depth: | 250 mm |
| Width with packaging: | 1.010 mm |
| Height with packaging: | 395 mm |
| Depth with packaging: | 300 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799513834 |
| Article number: | 0151.0383 |

Manufacturer: MAICO

LZP-R 28 External grille